                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 290605_A         Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 03/02/1992   Location: I-35 SB                       
        Pavement Width: 3.80 m.   Section Length: 305.00 m.
        Analysis Date: 08/19/1999 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     3.39     0.85     0.72
                   Total Slabs Distressed     -----      6.0      3.0      2.0

        Longitudinal Crack          METERS    -----     12.4      6.3     10.0
        ---Sealed---                METERS    -----      5.2        0        0

        Transverse Crack            METERS    -----     33.0     18.7     29.8
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     10.0      5.0      8.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      2.0      8.0     17.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      0.6      0.2      3.6

        Spall Trans. Joint          METERS    -----        0      5.0      2.6
                                    NUMBER    -----        0      5.0      4.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    265.4     26.9     11.1

        AC Patch                    SQ. M.    -----     0.27     0.62     0.61
                                    NUMBER    -----      1.0      2.0      2.0

        PCC Patch                   SQ. M.    -----    24.32    85.79    33.67
                                    NUMBER    -----      3.0      4.0      2.0

        Water Bleed & Pump          METERS     22.6    -----    -----    -----
                                    NUMBER     26.0    -----    -----    -----

        Transverse Joint            METERS     99.7    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

