                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 290661_A         Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 03/02/1992   Location: I-35 SB                       
        Pavement Width: 3.77 m.   Section Length: 152.50 m.
        Analysis Date: 08/24/1999 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0      1.0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      3.8        0      1.7
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     18.2        0     10.2
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      6.0        0      4.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0      7.0     16.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      4.7      5.7      4.8

        Spall Trans. Joint          METERS    -----      3.8      4.6      1.7
                                    NUMBER    -----      2.0      3.0      3.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    117.2     16.8     17.1

        AC Patch                    SQ. M.    -----     0.79     0.31     2.00
                                    NUMBER    -----      3.0      1.0      3.0

        PCC Patch                   SQ. M.    -----    46.60   103.13     9.24
                                    NUMBER    -----      7.0      3.0      1.0

        Water Bleed & Pump          METERS      8.3    -----    -----    -----
                                    NUMBER     12.0    -----    -----    -----

        Transverse Joint            METERS     85.5    -----    -----    -----
                                    NUMBER     23.0    -----    -----    -----

