                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 290663_a         Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 03/02/1992   Location: I-35 SB                       
        Pavement Width: 3.73 m.   Section Length: 152.50 m.
        Analysis Date: 08/24/1999 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0      2.1      5.8
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     23.9      0.9     14.5
        ---Sealed---                METERS    -----      7.5        0        0
                                    NUMBER    -----      8.0      1.0      4.0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      4.0      4.0     10.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      0.4      1.3      3.9

        Spall Trans. Joint          METERS    -----        0      0.5      1.2
                                    NUMBER    -----        0      1.0      2.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    121.6     21.9      8.3

        AC Patch                    SQ. M.    -----     0.36        0     1.17
                                    NUMBER    -----      2.0        0      2.0

        PCC Patch                   SQ. M.    -----    31.72    43.31    98.83
                                    NUMBER    -----      3.0      2.0      5.0

        Water Bleed & Pump          METERS      9.7    -----    -----    -----
                                    NUMBER     13.0    -----    -----    -----

        Transverse Joint            METERS     66.5    -----    -----    -----
                                    NUMBER     18.0    -----    -----    -----

