                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 290664_a         Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 03/02/1992   Location: I-35 SB                       
        Pavement Width: 3.86 m.   Section Length: 152.50 m.
        Analysis Date: 08/26/1999 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     2.21     1.05     0.60
                   Total Slabs Distressed     -----      3.0      3.0      1.0

        Longitudinal Crack          METERS    -----      2.0      9.1        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     34.6     11.1      2.8
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     11.0      3.0      1.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      3.0      4.0      7.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      3.2      1.0      1.7

        Spall Trans. Joint          METERS    -----      1.2      0.8      0.4
                                    NUMBER    -----      2.0      1.0      1.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    111.1     26.1     12.5

        AC Patch                    SQ. M.    -----        0     0.13     0.51
                                    NUMBER    -----        0      1.0      1.0

        PCC Patch                   SQ. M.    -----        0    92.67    10.10
                                    NUMBER    -----        0      3.0      2.0

        Water Bleed & Pump          METERS      7.9    -----    -----    -----
                                    NUMBER     10.0    -----    -----    -----

        Transverse Joint            METERS     52.1    -----    -----    -----
                                    NUMBER     14.0    -----    -----    -----

