                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 295000           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 10/18/2002   Location: I-35 NB                       
        Pavement Width: 3.77 m.   Section Length: 152.50 m.
        Analysis Date: 11/06/2002 Operator Name: ECH                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----     0.56        0        0
                   Total Slabs Distressed     -----      1.0        0        0

        Longitudinal Crack          METERS    -----      1.6        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     29.5      0.6      6.0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      8.0      1.0      2.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      2.0      0.3     18.8

        Spall Trans. Joint          METERS    -----        0      1.1        0
                                    NUMBER    -----        0      1.0        0

        Map Cracking                SQ. M.     3.42    -----    -----    -----
                                    NUMBER      3.0    -----    -----    -----

        Scaling                     SQ. M.     0.18    -----    -----    -----
                                    NUMBER      2.0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    149.1        0        0

        AC Patch                    SQ. M.    -----     0.09     0.40     0.34
                                    NUMBER    -----      1.0      2.0      2.0

        PCC Patch                   SQ. M.    -----    32.70     3.44     0.19
                                    NUMBER    -----      7.0      5.0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     48.6    -----    -----    -----
                                    NUMBER     13.0    -----    -----    -----

