                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 03/10/1993   Location: I-35 SB                       
        Pavement Width: 3.74 m.   Section Length: 305.00 m.
        Analysis Date: 04/02/1998 Operator Name: SMF                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      3.6        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      8.6        0        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      3.0        0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     25.0        0      2.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     19.4      0.2      1.3

        Spall Trans. Joint          METERS    -----      8.0      3.0      0.7
                                    NUMBER    -----      5.0      3.0      1.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.6        0        0

        AC Patch                    SQ. M.    -----     0.34        0        0
                                    NUMBER    -----      1.0        0        0

        PCC Patch                   SQ. M.    -----    33.30     8.22     8.20
                                    NUMBER    -----      7.0      2.0      2.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     99.8    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

