                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 01/11/2004   Location: I-35 SB                       
        Pavement Width: 3.64 m.   Section Length: 305.00 m.
        Analysis Date: 04/05/2004 Operator Name: PDE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     24.1      3.2      1.8
        ---Sealed---                METERS    -----      6.9        0        0

        Transverse Crack            METERS    -----     44.2      1.4        0
        ---Sealed---                METERS    -----      0.7        0        0
                                    NUMBER    -----     24.0      1.0        0
        ---Sealed---                NUMBER    -----      1.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----        0        0      3.3

        Spall Trans. Joint          METERS    -----        0        0     14.0
                                    NUMBER    -----        0        0      7.0

        Map Cracking                SQ. M.    13.15    -----    -----    -----
                                    NUMBER      3.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   350.14    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    299.4      1.0        0

        AC Patch                    SQ. M.    -----        0     0.25     2.09
                                    NUMBER    -----        0      1.0      7.0

        PCC Patch                   SQ. M.    -----     4.56        0    49.50
                                    NUMBER    -----      1.0        0      9.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     97.6    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

