                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400602           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 11/18/2001   Location: I-35 SB                       
        Pavement Width: 3.73 m.   Section Length: 305.00 m.
        Analysis Date: 01/31/2002 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     20.0      3.0      2.6
        ---Sealed---                METERS    -----      1.0        0        0

        Transverse Crack            METERS    -----     69.3        0      0.8
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----     30.0        0      1.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----        0      0.5      2.3

        Spall Trans. Joint          METERS    -----      0.3        0     10.7
                                    NUMBER    -----        0        0      6.0

        Map Cracking                SQ. M.     2.71    -----    -----    -----
                                    NUMBER      3.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    305.7        0        0

        AC Patch                    SQ. M.    -----     0.19     0.34     1.29
                                    NUMBER    -----      1.0      1.0      5.0

        PCC Patch                   SQ. M.    -----     4.33        0    48.20
                                    NUMBER    -----      1.0        0      9.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     99.9    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

