                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 11/18/2001   Location: I-35 SB                       
        Pavement Width: 3.69 m.   Section Length: 305.00 m.
        Analysis Date: 02/01/2002 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     42.3      0.9      0.5
        ---Sealed---                METERS    -----     21.8        0        0

        Transverse Crack            METERS    -----     63.3      0.7        0
        ---Sealed---                METERS    -----      7.3        0        0
                                    NUMBER    -----     20.0      1.0        0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----        0      0.9      3.2

        Spall Trans. Joint          METERS    -----      1.2      1.4     19.7
                                    NUMBER    -----      1.0      1.0      9.0

        Map Cracking                SQ. M.  1070.12    -----    -----    -----
                                    NUMBER     12.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    302.8        0        0

        AC Patch                    SQ. M.    -----     1.06     0.25     9.63
                                    NUMBER    -----      4.0      1.0      8.0

        PCC Patch                   SQ. M.    -----     4.42        0    30.90
                                    NUMBER    -----      1.0        0      6.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     95.2    -----    -----    -----
                                    NUMBER     26.0    -----    -----    -----

