                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 10/28/1991   Location: I-35 SB                       
        Pavement Width: 3.79 m.   Section Length: 305.00 m.
        Analysis Date: 07/19/1999 Operator Name: DEE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     17.1      2.2      1.0
        ---Sealed---                METERS    -----      0.6        0        0

        Transverse Crack            METERS    -----     18.0      3.8        0
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      4.0      1.0        0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----      5.0     11.0      3.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      0.4      1.6      2.2

        Spall Trans. Joint          METERS    -----      2.0      1.4     11.6
                                    NUMBER    -----      2.0      1.0      7.0

        Map Cracking                SQ. M.   251.60    -----    -----    -----
                                    NUMBER     30.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    303.2        0        0

        AC Patch                    SQ. M.    -----     0.40        0     2.97
                                    NUMBER    -----      2.0        0      4.0

        PCC Patch                   SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     70.4    -----    -----    -----
                                    NUMBER     19.0    -----    -----    -----

