                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 400605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 01/11/2004   Location: I-35 SB                       
        Pavement Width: 3.76 m.   Section Length: 305.00 m.
        Analysis Date: 04/07/2004 Operator Name: PDE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----     27.0        0        0
        ---Sealed---                METERS    -----     17.6        0        0

        Transverse Crack            METERS    -----     71.2        0        0
        ---Sealed---                METERS    -----      5.0        0        0
                                    NUMBER    -----     22.0        0        0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----        0        0      4.7

        Spall Trans. Joint          METERS    -----      0.7        0     21.6
                                    NUMBER    -----      1.0        0     10.0

        Map Cracking                SQ. M.  1080.36    -----    -----    -----
                                    NUMBER     20.0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.   351.32    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    300.6      5.9        0

        AC Patch                    SQ. M.    -----     1.75        0    14.42
                                    NUMBER    -----      7.0        0     13.0

        PCC Patch                   SQ. M.    -----     4.61        0    31.04
                                    NUMBER    -----      2.0        0      8.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     96.7    -----    -----    -----
                                    NUMBER     26.0    -----    -----    -----

