                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 420605           Pavement Type: Jointed Reinforced Concrete   
        Survey Date: 08/02/1999   Location: I-80 WB                       
        Pavement Width: 3.69 m.   Section Length: 305.00 m.
        Analysis Date: 09/30/1999 Operator Name: KAE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      1.8        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      3.9      2.0      5.8
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      2.0      1.0      4.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     16.0      4.0      7.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----    220.5      6.0      3.8

        Spall Trans. Joint          METERS    -----      7.5      2.9      6.2
                                    NUMBER    -----      7.0      3.0      5.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    101.0     80.7    125.0

        AC Patch                    SQ. M.    -----        0        0     4.84
                                    NUMBER    -----        0        0     11.0

        PCC Patch                   SQ. M.    -----    87.88    35.78     0.47
                                    NUMBER    -----     10.0      1.0      2.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS     94.2    -----    -----    -----
                                    NUMBER     27.0    -----    -----    -----

