                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460601           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 09/27/2001   Location: US-12 WB                      
        Pavement Width: 3.75 m.   Section Length: 152.50 m.
        Analysis Date: 11/16/2001 Operator Name: KAE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0      1.0

        Durability Cracking         SQ. M.    -----    47.53     4.12     1.70
                   Total Slabs Distressed     -----     19.0      7.0      3.0

        Longitudinal Crack          METERS    -----     29.0      7.7      1.0
        ---Sealed---                METERS    -----      0.7        0        0

        Transverse Crack            METERS    -----     24.3      6.3      3.7
        ---Sealed---                METERS    -----      1.1        0        0
                                    NUMBER    -----     20.0      3.0      2.0
        ---Sealed---                NUMBER    -----      3.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      0.3      1.4      1.5

        Spall Trans. Joint          METERS    -----      9.9        0     14.7
                                    NUMBER    -----      6.0        0      9.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----     92.5     38.4     16.0

        AC Patch                    SQ. M.    -----     3.04     2.18    10.73
                                    NUMBER    -----     10.0      2.0      7.0

        PCC Patch                   SQ. M.    -----    44.33        0    30.44
                                    NUMBER    -----      7.0        0      2.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    113.8    -----    -----    -----
                                    NUMBER     30.0    -----    -----    -----

