                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460601           Pavement Type: Jointed Plain Concrete        
        Survey Date: 08/20/1999   Location: US-12 WB                      
        Pavement Width: 3.72 m.   Section Length: 152.50 m.
        Analysis Date: 11/15/1999 Operator Name: MJE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0        0      1.0

        Durability Cracking         SQ. M.    -----     5.19    12.27    25.89
                   Total Slabs Distressed     -----      4.0      6.0     12.0

        Longitudinal Crack          METERS    -----     34.3        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----      5.3        0      0.3
        ---Sealed---                METERS    -----        0        0        0
                                    NUMBER    -----      7.0        0      1.0
        ---Sealed---                NUMBER    -----        0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     26.0      2.0      2.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      1.0        0        0

        Spall Trans. Joint          METERS    -----      1.8      0.4        0
                                    NUMBER    -----      1.0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    105.9     11.1     32.5

        AC Patch                    SQ. M.    -----     1.27        0     0.86
                                    NUMBER    -----      5.0        0      1.0

        PCC Patch                   SQ. M.    -----    42.78    29.48        0
                                    NUMBER    -----      9.0      1.0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    112.2    -----    -----    -----
                                    NUMBER     30.0    -----    -----    -----

