                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460601           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 07/24/2003   Location: US-12 WB                      
        Pavement Width: 3.81 m.   Section Length: 152.50 m.
        Analysis Date: 10/13/2003 Operator Name: KAE                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0      2.0

        Durability Cracking         SQ. M.    -----    87.15     7.95     2.20
                   Total Slabs Distressed     -----     21.0      6.0      1.0

        Longitudinal Crack          METERS    -----     69.8      7.4      6.6
        ---Sealed---                METERS    -----      1.7        0        0

        Transverse Crack            METERS    -----     29.2     22.1     12.5
        ---Sealed---                METERS    -----      1.0        0        0
                                    NUMBER    -----     22.0     12.0      7.0
        ---Sealed---                NUMBER    -----      3.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      4.6      0.9      3.9

        Spall Trans. Joint          METERS    -----      7.6      1.2     27.3
                                    NUMBER    -----      5.0      1.0     14.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----     74.2     37.8     44.3

        AC Patch                    SQ. M.    -----     1.79     1.39    15.85
                                    NUMBER    -----      7.0      4.0     15.0

        PCC Patch                   SQ. M.    -----    44.51        0    30.69
                                    NUMBER    -----      8.0        0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    114.9    -----    -----    -----
                                    NUMBER     31.0    -----    -----    -----

