                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460601           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 07/23/2002   Location: US-12 WB                      
        Pavement Width: 3.80 m.   Section Length: 152.50 m.
        Analysis Date: 08/09/2002 Operator Name: MMW                           
        Section Start : 0.00 m.   Section End   : 152.50 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0      2.0

        Durability Cracking         SQ. M.    -----    55.52    13.69     1.04
                   Total Slabs Distressed     -----     11.0     16.0        0

        Longitudinal Crack          METERS    -----     25.2     10.5      1.6
        ---Sealed---                METERS    -----      0.9        0        0

        Transverse Crack            METERS    -----     21.4     10.3      4.8
        ---Sealed---                METERS    -----      0.5        0        0
                                    NUMBER    -----     19.0      5.0      4.0
        ---Sealed---                NUMBER    -----      2.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----      1.9      1.3      2.2

        Spall Trans. Joint          METERS    -----      4.0        0     22.6
                                    NUMBER    -----      2.0        0     14.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----     88.3     34.8     28.8

        AC Patch                    SQ. M.    -----     1.37     3.43    15.32
                                    NUMBER    -----      7.0      3.0     13.0

        PCC Patch                   SQ. M.    -----    43.39        0    31.03
                                    NUMBER    -----      7.0        0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    115.4    -----    -----    -----
                                    NUMBER     30.0    -----    -----    -----

