                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 07/23/2002   Location: US-12 WB                      
        Pavement Width: 3.82 m.   Section Length: 305.00 m.
        Analysis Date: 08/08/2002 Operator Name: MMW                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      5.0      4.0      6.0

        Durability Cracking         SQ. M.    -----    11.58     0.20        0
                   Total Slabs Distressed     -----     18.0      1.0        0

        Longitudinal Crack          METERS    -----    140.0      8.1      0.3
        ---Sealed---                METERS    -----     33.1        0        0

        Transverse Crack            METERS    -----     63.5     16.7        0
        ---Sealed---                METERS    -----     42.7        0        0
                                    NUMBER    -----     61.0     11.0        0
        ---Sealed---                NUMBER    -----     42.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      5.9     11.6     20.2

        Spall Trans. Joint          METERS    -----      0.5      0.4     31.6
                                    NUMBER    -----      1.0      1.0     23.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----      1.0    137.8    166.7

        AC Patch                    SQ. M.    -----     3.78     1.81    10.48
                                    NUMBER    -----     11.0      5.0     16.0

        PCC Patch                   SQ. M.    -----    48.60    29.93     3.29
                                    NUMBER    -----     22.0      2.0      3.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    217.3    -----    -----    -----
                                    NUMBER     57.0    -----    -----    -----

