                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 07/24/2003   Location: US-12 WB                      
        Pavement Width: 3.79 m.   Section Length: 305.00 m.
        Analysis Date: 10/03/2003 Operator Name: TLE                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      6.0      6.0      6.0

        Durability Cracking         SQ. M.    -----    18.11     0.96     0.12
                   Total Slabs Distressed     -----     17.0      2.0      1.0

        Longitudinal Crack          METERS    -----    160.5     12.5      1.5
        ---Sealed---                METERS    -----     33.3        0        0

        Transverse Crack            METERS    -----     73.1     33.3      7.2
        ---Sealed---                METERS    -----     39.2        0        0
                                    NUMBER    -----     68.0     22.0      5.0
        ---Sealed---                NUMBER    -----     41.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     37.5     10.8     18.2

        Spall Trans. Joint          METERS    -----      2.2      0.6     41.4
                                    NUMBER    -----      2.0      1.0     31.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----     15.6    128.8    160.3

        AC Patch                    SQ. M.    -----     2.48     3.11    11.09
                                    NUMBER    -----     11.0      9.0     22.0

        PCC Patch                   SQ. M.    -----    47.67    30.95     0.98
                                    NUMBER    -----     23.0      5.0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    216.6    -----    -----    -----
                                    NUMBER     57.0    -----    -----    -----

