                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460605           Pavement Type: Jointed Plain Concrete        
        Survey Date: 06/18/1996   Location: US-12 WB                      
        Pavement Width: 3.84 m.   Section Length: 305.00 m.
        Analysis Date: 08/28/1997 Operator Name: LRL                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----      7.1        0        0
        ---Sealed---                METERS    -----      7.1        0        0

        Transverse Crack            METERS    -----     21.2        0        0
        ---Sealed---                METERS    -----     19.6        0        0
                                    NUMBER    -----     48.0        0        0
        ---Sealed---                NUMBER    -----     44.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----     54.0        0      3.0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      1.0    -----    -----    -----

        Spall Long. Joint           METERS    -----     13.0      0.6      1.3

        Spall Trans. Joint          METERS    -----      1.0      0.5        0
                                    NUMBER    -----      1.0      1.0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    303.0        0        0

        AC Patch                    SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        PCC Patch                   SQ. M.    -----    51.82    29.60        0
                                    NUMBER    -----     25.0      2.0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    215.2    -----    -----    -----
                                    NUMBER     57.0    -----    -----    -----

