                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 460605           Pavement Type: Planned AC Overlay of JCP     
        Survey Date: 09/27/2001   Location: US-12 WB                      
        Pavement Width: 3.73 m.   Section Length: 305.00 m.
        Analysis Date: 11/15/2001 Operator Name: HMW                           
        Section Start : 0.00 m.   Section End   : 305.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----      1.0      4.0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----    102.4      1.7      0.3
        ---Sealed---                METERS    -----     35.2        0        0

        Transverse Crack            METERS    -----     56.4      4.6      1.5
        ---Sealed---                METERS    -----     45.0        0        0
                                    NUMBER    -----     59.0      3.0      2.0
        ---Sealed---                NUMBER    -----     46.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER        0    -----     -----     -----

        Spall Long. Joint           METERS    -----     12.8      7.3     13.9

        Spall Trans. Joint          METERS    -----      1.5      0.5     24.7
                                    NUMBER    -----      2.0      1.0     22.0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----     23.3    114.8    167.7

        AC Patch                    SQ. M.    -----     2.13     4.18     3.92
                                    NUMBER    -----      9.0      9.0      6.0

        PCC Patch                   SQ. M.    -----    48.52    30.03     1.31
                                    NUMBER    -----     25.0      2.0      1.0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    214.5    -----    -----    -----
                                    NUMBER     57.0    -----    -----    -----

