                                SECTION SUMMARY                       
                       PADIAS REPORT GENERATOR - REV. 4.0

        Section: 49D446           Pavement Type: Jointed Plain Concrete        
        Survey Date: 09/12/2002   Location: ST-154 SB                     
        Pavement Width: 3.84 m.   Section Length: 122.00 m.
        Analysis Date: 10/04/2002 Operator Name: MMW                           
        Section Start : 0.00 m.   Section End   : 122.00 m. 

        Distress Type                     Reduced Extent at Each Severity

        _________________________   Unit___ No Sev.___ Low____ Mod.____ High___

        Corner Breaks               NUMBER    -----        0        0        0

        Durability Cracking         SQ. M.    -----        0        0        0
                   Total Slabs Distressed     -----        0        0        0

        Longitudinal Crack          METERS    -----        0        0        0
        ---Sealed---                METERS    -----        0        0        0

        Transverse Crack            METERS    -----     15.7        0        0
        ---Sealed---                METERS    -----      3.8        0        0
                                    NUMBER    -----      5.0        0        0
        ---Sealed---                NUMBER    -----      1.0        0        0

        Tran. Jt. Seal Dmg.  SEALED JOINTS      YES
                                    NUMBER    -----        0        0        0

        Long. Jt. Seal Dmg.         METERS        0    -----    -----    -----
        ---Sealed---                NUMBER      2.0    -----    -----    -----

        Spall Long. Joint           METERS    -----      5.5        0        0

        Spall Trans. Joint          METERS    -----      0.8        0        0
                                    NUMBER    -----      1.0        0        0

        Map Cracking                SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Scaling                     SQ. M.        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Polished Aggregate          SQ. M.        0    -----    -----    -----

        Blowups                     NUMBER        0    -----    -----    -----

        Lane-Shoulder Sep.          METERS    -----    119.5        0        0

        AC Patch                    SQ. M.    -----        0        0        0
                                    NUMBER    -----        0        0        0

        PCC Patch                   SQ. M.    -----     4.22(0.0)   0        0
                                    NUMBER    -----      3.0(0.0)   0        0

        Water Bleed & Pump          METERS        0    -----    -----    -----
                                    NUMBER        0    -----    -----    -----

        Transverse Joint            METERS    121.2    -----    -----    -----
                                    NUMBER     32.0    -----    -----    -----

Edge drains rated as patches have been removed.
