# Technical Specifications

TapeDeck records compressed AAC audio at the following settings:

- High Quality - 44,100Hz, 16-bit, 64kbps (mono) or 128kbps (stereo)
- Medium Quality - 44,100Hz, 16-bit, 48kbps (mono) or 96kbps (stereo)
- Low Quality - 22,050Hz, 16-bit, 32kbps (mono) or 64kbps (stereo)

Note: When recording with an advanced audio device with >2 channels of input, TapeDeck only records using the first 2 channels in stereo mode, or the first channel in mono mode.