****************************************************************************
 HDVR Integration for C•CURE 9000 Version 2.02 April 2012
 Copyright © 2012 Tyco International Ltd. and its Respective Companies.
****************************************************************************

This readme file provides important information about the HDVR Integration for C•CURE 9000 Version 2.02. Please read this file before installing the product.

************************************************************
*  Product: C•CURE 9000 HDVR Integration Software
*  Release: Upgrade Release
*  Version: 2.02 Build 4630
*  HDVR Server version: 1.4,1.5,1.6
*  HDVR evAPI version: 1.11
*  Company: Software House (Tyco International)
*  Date: January 13, 2012

************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************
This document contains the following sections:

1. Overview
2. Features
3. Hardware Requirements
4. Software Requirements
5. Qualified Operating Systems
6. Qualified Hardware/Software
7. Contents of the Installation Kit
8. Pre-installation
9. Installation
10. Post-installation
11. Issues and Limitations

************************************************************
* 1. OVERVIEW
************************************************************

HDVR integration is a C•CURE 9000 integration application which can configure HDVR video server and video camera. User can show video view,
video tour, do PTZ controls and trigger alarm events or camera actions when camera has alarm.

************************************************************
* 2. FEATURES
************************************************************

The C•CURE 9000 HDVR Integration software offers the following features:

 • Live video
 • Simultaneous live and recorded video views from up to 16 cameras
 • Export of video to avi and ps format
 • Playback of pre-recorded video
 • Video control such as PTZ (domes only)
 • Video tours
 • Video alarms
 • PTZ presets based on event, alarm input or video tour
  
************************************************************
* 3. HARDWARE REQUIREMENTS 
************************************************************

HDVR Integration has the same hardware, software, and disk space requirements as C•CURE 9000; if the target computer can install C•CURE 9000, then it satisfies HDVR Integration requirements.

************************************************************
* 4. SOFTWARE REQUIREMENTS 
************************************************************

The C•CURE 9000 HDVR Integration requires the following software versions:

 • Exacq API version :1.11
 • HDVR Server version: 1.4,1.5,1.6
 • C•CURE 9000 Security and Event Management System version 2.02 Build 4630.


 NOTE: The HDVR integration server components cannot be installed on a MAS.

       Close any running applications to avoid installation problems.

************************************************************

************************************************************
* 5. QUALIFIED OPERATING SYSTEMS
************************************************************

32-bit operating systems:

 • Windows XP Service Pack 3
 • Windows 2003 Service Pack 2
 • Windows 2008  
 • Windows 7 Professional

64-bit operating systems are not supported by HDVR evAPI v1.9.0.22273.
 • Windows 2008 R2 
 • Windows 7 Professional



************************************************************
* 6. QUALIFIED HARDWARE/SOFTWARE
************************************************************

 • Exacq API version 1.11
 • HDVR Software version 1.4,1.5,1.6
 • IP cameras: ApproM, Axis213, Axis214, Arecont AV1300, Panasonic WV-NS202A, Sony SNC-DF80P
 • Analog camera: ADCA470CAFP


************************************************************
* 7. CONTENTS OF THE INSTALLATION KIT
************************************************************
 
 The C•CURE 9000 HDVR Integration software package contains the following items:

 • HDVR Integration User Guide.pdf - C•CURE 9000 (version 2.0) HDVR Integration Software User Guide
 • CCURE9000_HDVR_Integration_readme.txt - C•CURE 9000 HDVR Integration Software ReadMe file
 • CCURE_9000_HDVR_Integration.exe - HDVR Integration software setup file

************************************************************
* 8. PRE-INSTALLATION
************************************************************

To perform the installation, you must have appropriate Windows permissions. You must have membership in the local Administrators group, or equivalent privileges. See the Microsoft Operating System document or your system administrator for more information.

************************************************************
* 9. INSTALLATION
************************************************************

Perform the following steps to install the C•CURE 9000 HDVR Integration:

Note: You must install the HDVR Integration in the same folder as C•CURE 9000 v2.02. Also, you must have administrator privileges to do the 
      install. Otherwise the system displays the error message: "The system administrator has set policies to prevent this installation."

 1. Double-click the CCURE_9000_HDVR_Integration.exe file.
 2. The installation program determines if the correct version of C•CURE 9000 is installed on your system, and if it is not, a message is displayed 
    stating that a supported version of C•CURE 9000 is needed.
 3. The Install Wizard begins installing the software, and the HDVR Integration Welcome screen appears.
 4. Click Next and follow the Install Wizard prompts.   
 5. Click Finish to complete the Installation, and use the Server Management Application to start the Crossfire Service.
 6. Open the HDVR Integration User Guide.pdf and read the guide for information about using the C•CURE 9000 HDVR Integration product. 

************************************************************
* 10. POST-INSTALLATION
************************************************************

 1. From the Start Menu, select Start>All Programs>Software House>Server Configuration to open the C•CURE 9000 Server Management Application.
 2. Restart the CrossFire services and the Server Component Framework services.
 3. Verify the license for the HDVR Integration by running C•CURE 9000 Licensing utility on the C•CURE 9000 server.
 4. Under Server Components tab, right-click ConnectedPro.HardwareInterface.HDVR.HardwareInterface Integration Interface under Video and select Start Server Component from the context menu.
 5. When the server component icon for HDVR Integration changes from Disabled (Red) to Enabled (Green), you can use the HDVR Integration software.

You can also install C•CURE 9000 HDVR Integration software on a local computer either from a shared drive or over a network.   

************************************************************
* 11. ISSUES AND LIMITATIONS
************************************************************

 • The HDVR Integration works on following 32-bit OS depending on turning off DEP by command "bcdedit /set nx alwaysoff":
 	Windows Server 2008, Windows 7 and Vista(only client) Operation systems. 
 • If the video size is more than 20G, it is recommended to retrieve video clips by splitting the video. 
 • No support exporting video more than 2G per file.
 • On Windows 7 and window2008, the database tables may not be dropped during uninstallation. This must be done manually.

************************************************************

Copyright and Trademarks
C•CURE and Software House are registered trademarks of Tyco International Ltd. 
and its respective Companies.

The trademarks, logos, and service marks displayed on this document are registered 
in the United States [or other countries]. Any misuse of the trademarks is strictly 
prohibited and Tyco International Ltd. will aggressively enforce its intellectual 
property rights to the fullest extent of the law, including pursuit of criminal 
prosecution wherever necessary. All trademarks not owned by Tyco International Ltd. 
are the property of their respective owners, and are used with permission or allowed 
under applicable laws.

Product offerings and specifications are subject to change without notice. Actual 
products may vary from photos. Not all products include all features. Availability 
varies by region; contact your regional sales manager.

Software version: C•CURE 9000 version 2.02.
Print Date: January, 2012

This manual is proprietary information of Software House. Unauthorized reproduction 
of any portion of this manual is prohibited. The material in this manual is for 
information purposes only. It is subject to change without notice. Software House 
assumes no responsibility for incorrect information this manual may contain.

All rights reserved.
Copyright © 2011 Tyco International Ltd. and its Respective Companies.

***********************************************************************************

End of ReadMe File


