# Uses of Package
com.jscape.inet.terminal.commands

- Packages that use com.jscape.inet.terminal.commands
  Package | Description
  --- | ---
  com.jscape.inet.terminal |
  com.jscape.inet.terminal.commands |

- Classes in com.jscape.inet.terminal.commands used by com.jscape.inet.terminal
  Class and Description
  ControlCommand Base interface for control commands.

- Classes in com.jscape.inet.terminal.commands used by com.jscape.inet.terminal.commands
  Class and Description
  AMCommand Exit Graphics Mode.
  ANSICommand Enter ANSI Mode.
  BSCommand Move the cursor to the left one character position, unless it is at the left margin, in which case no action occurs.
  CANCommand If sent during a control sequence, the sequence is immediately terminated and not executed.
  ControlCommand Base interface for control commands.
  CPRCommand CPR -- Cursor Position Report.
  CRCommand Move cursor to the left margin on the current line.
  CUBCommand CUB -- Cursor Backward.
  CUDCommand CUD -- Cursor Down.
  CUFCommand CUF -- Cursor Forward.
  CUHCommand Cursor to Home.
  CUPCommand CUP -- Cursor Position.
  CUUCommand CUU -- Cursor Up.
  DACommand DA -- Device Attributes.
  DECIDCommand DECID -- Identify Terminal.
  DECSTBMCommand DECSTBM -- Set Top and Bottom Margins.
  DECTSTCommand DECTST -- Invoke Confidence Test.
  DSRCommand DSR -- Device Status Report.
  EDCommand ED -- Erase In Display.
  EELCommand Erase to End of Line.
  EESCommand Erase to End of Screen.
  ELCommand EL -- Erase In Line.
  ESCCommand Invokes a control sequence.
  GMCommand Enter Graphics Mode.
  HTCommand Move the cursor to the next tab stop, or to the right margin if no further tab stops are present on the line.
  HTSCommand HTS -- Horizontal Tabulation Set.
  INDCommand IND -- Index.
  LFCommand This command causes a line feed or a new line operation.
  NELCommand NEL -- Next Line.
  NullCommand Defines null action.
  RICommand RI -- Reverse Index.
  RMCommand RM -- Reset Mode.
  SCSG00Command SCS -- Select Character Set.
  SCSG0BCommand SCS -- Select Character Set.
  SCSG10Command SCS -- Select Character Set.
  SCSG1BCommand SCS -- Select Character Set.
  SGRCommand SGR -- Select Graphic Rendition.
  SICommand Select G0 character set, as selected by "ESC (" sequence.
  SMCommand SM -- Set Mode.
  SOCommand Invoke G1 character set, as designated by SCS control sequence.
  TBCCommand

Copyright © JSCAPE LLC. 1999-2021. All Rights Reserved