# Package com.jscape.inet.terminal.commands

- Interface Summary
  Interface | Description
  --- | ---
  ControlCommand | Base interface for control commands.

- Class Summary
  Class | Description
  --- | ---
  AMCommand | Exit Graphics Mode.
  ANSICommand | Enter ANSI Mode.
  BSCommand | Move the cursor to the left one character position, unless it is at the left margin, in which case no action occurs.
  CANCommand | If sent during a control sequence, the sequence is immediately terminated and not executed.
  CPRCommand | CPR -- Cursor Position Report.
  CRCommand | Move cursor to the left margin on the current line.
  CUBCommand | CUB -- Cursor Backward.
  CUDCommand | CUD -- Cursor Down.
  CUFCommand | CUF -- Cursor Forward.
  CUHCommand | Cursor to Home.
  CUPCommand | CUP -- Cursor Position.
  CUUCommand | CUU -- Cursor Up.
  DACommand | DA -- Device Attributes.
  DECIDCommand | DECID -- Identify Terminal.
  DECSTBMCommand | DECSTBM -- Set Top and Bottom Margins.
  DECTSTCommand | DECTST -- Invoke Confidence Test.
  DSRCommand | DSR -- Device Status Report.
  EDCommand | ED -- Erase In Display.
  EELCommand | Erase to End of Line.
  EESCommand | Erase to End of Screen.
  ELCommand | EL -- Erase In Line.
  ESCCommand | Invokes a control sequence.
  GMCommand | Enter Graphics Mode.
  HTCommand | Move the cursor to the next tab stop, or to the right margin if no further tab stops are present on the line.
  HTSCommand | HTS -- Horizontal Tabulation Set.
  INDCommand | IND -- Index.
  LFCommand | This command causes a line feed or a new line operation.
  NELCommand | NEL -- Next Line.
  NullCommand | Defines null action.
  RICommand | RI -- Reverse Index.
  RMCommand | RM -- Reset Mode.
  SCSG00Command | SCS -- Select Character Set.
  SCSG0BCommand | SCS -- Select Character Set.
  SCSG10Command | SCS -- Select Character Set.
  SCSG1BCommand | SCS -- Select Character Set.
  SGRCommand | SGR -- Select Graphic Rendition.
  SICommand | Select G0 character set, as selected by "ESC (" sequence.
  SMCommand | SM -- Set Mode.
  SOCommand | Invoke G1 character set, as designated by SCS control sequence.
  TBCCommand |

Copyright © JSCAPE LLC. 1999-2021. All Rights Reserved