System Requirements

# System Requirements: Itanium®-based Computers

Before installing the Intel® 10GbE Server Adapter, check your system for the following minimum configuration requirements.

## Hardware Compatibility

- Itanium®-based computer

- The latest BIOS for your system

- One of the following slot types, depending on your adapter:

  - PCI-X slot (v1.0a compliant), 3.3v PCI-X signaling, operating at 66, 100 or 133 MHz

  - PCI bus master slot (v2.3 compliant), 3.3v PCI signaling, 32- or 64-bit, operating at 33 or 66 MHz

  - One open PCI-Express slot (v1.0a or newer), 8x or 16x.

## Supported 64-bit Operating Systems

The Intel drivers for Itanium-based systems operate with the following operating systems:

- Microsoft Windows* Server 2003, 64-Bit Edition (Enterprise Server or Datacenter Server versions), with latest service pack installed

- Microsoft Windows Server 2008 for Itanium-based Systems, with the latest service pack installed

- Microsoft Windows Server 2008 R2

- Linux, v2.x kernel and higher, except v2.6

`Last modified on 7/23/09 1:41p Revision 15`