2011 LIEBHERR R954BHDW EXCAVATOR MATERIAL HANDLER WITH BATEMAN MAGGRAB

Year: 2011

Brand: Liebherr (Excavator) / Bateman (Maggrab)

Model: R954BHDW Litronic (Excavator) / BMG16-150M40 (Maggrab)

Hours: 40,172 hours accurate/verified

General Specifications:

Operating Weight: Approximately 56.9 metric tons (56,900 kg)

Engine: Liebherr D926 TI-E

Type: 6-cylinder, turbocharged, direct injection, after-cooled

Displacement: 10 liters

Power: 222 kW (approximately 297 hp) at 2,000 rpm

Track: Triple Grouser Track Shoes

Track Width: 750 mm

Track Condition: New

Cab: Enclosed cab a/c 7 heat

Interface: can screen

Control: 22’4” stick

Bateman Maggrab:

Bateman - BMG16-150M40 Maggrab

Series: 160

Capacity: 1.15 (Cubic meters)

Magnet Diameter: 40'' inches

Weight: 7750 lbs

Tip to Tip Width: 124'' inches

Height (open Tines): 80'' inches

Height (Closed Tines): 115'' inches

Operational Capacities:

Fuel Tank: 706 liters

Hydraulic System Fluid Capacity: 800 liters

Performance:

Maximum Digging Depth: 9 meters

Maximum Reach: 9 meters

Tear-Out Force: 285 kN

Swing Mechanism:

Swing Speed: 6.2 rpm

Swing Torque: 156,000 Nm

Hydraulics:

Pump Type: Variable displacement swash plate

Pump Capacity: Up to 700 L/min

System Pressure: 35,000 kPa

Operating Weight: Approximately 52,000 kg