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ARRANGEMENTS AND PROCEDURES


Policy Statement:

[bookmark: _Hlk140232471]This Tyre Management Policy has been established by <<Business Name>> to prioritise safety and compliance in all aspects of our operations. This Tyre Policy is designed to outline the guidelines and procedures regarding tyres and their maintenance. Adhering to these guidelines ensures the safety of our drivers, vehicles, and the public, while also minimising the risk of costly accidents and vehicle downtime.

1. Scope and Applicability
This policy applies to all managers, drivers and other employees of our transport company. It is the responsibility of the Transport Manager to oversee and manage all aspects of Tyre Management, ensuring that compliance is monitored, assessed and rectified as appropriate.

2. Responsibility
The condition of tyres represent a major part of vehicle roadworthiness. Tyres affect the handling, stability and braking of a vehicle and are the only point of contact between the vehicle and the road. As such,  <<Business Name>> takes the responsibility of tyre management very seriously.

When a driver takes a vehicle out on the public highway, they assume partial responsibility for the condition of the tyres. Part of a driver’s vehicle checks include checking the condition and security of the tyres. Failure to carry this out diligently, or to take a vehicle onto the public road with a defective tyre, will result in the driver receiving stiff penalties from DVSA should a tyre be bald or worn. This is in addition to any company sanctions.

Tyre maintenance will be handled primarily by <<Insert Tyre Company Name>>, who will assume responsibility for wheel removal, tyre replacement, refitting of wheel and ensuring the wheel nuts are torqued to the correct level.

3. Legal Minimum Requirements and Company Policies
· The minimum tread depth under legislation is 1.0mm. Company policy is that no tyre should be used where tread depth falls below a minimum of 3.0mm
· The tread depth is measured across three quarters of the tread and around the entire circumference of the tyre. The balance of the tyre that is not falling within the three quarters must have visible grooves.
· Tyres will not be used where they show signs of a lump bulge or tyre 
· Tyre inflation will be checked at inspection and service. Visual checks will be made during a driver vehicle check.
· The age of the tyre will be checked to ensure compliance with the 10 year age limit rules.
· A wheel that has been removed from the vehicle and refitted must be tightened to the correct torque.
· The company re-torque policy is that the torque settings are checked by the tyre company after the vehicle has been left stationary for 30 minute.
· Safe disposal of used tyre casing s will be organised by the tyre contractor.


4. Policy Responsibility and Review
· [bookmark: Text63]Overall responsibility for this Tyre Management Policy within <<Business name>> and the implementation thereof lies with <<insert name and position / department etc.>>.
· This Tyre Management Policy is regularly reviewed and updated as required.
· [bookmark: Text60]This Tyre Management Policy was adopted on <<insert date>>.
· [bookmark: Text61]This Tyre Management Policy was last reviewed on <<insert date>>.
· This Tyre Management Policy will be reviewed, on <<insert date>>
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