GSSHA_INDEX_MAP_TABLES
INDEX_MAP                "C:\A_Aquaveo\Training\GSSHA\Calibration\Manual\id_map_1.idx" "Index Map - 1"
INDEX_MAP                "C:\A_Aquaveo\Training\GSSHA\Calibration\Manual\id_map_2.idx" "land use"
INDEX_MAP                "C:\A_Aquaveo\Training\GSSHA\Calibration\Manual\id_map_3.idx" "lusoil"
INDEX_MAP                "C:\A_Aquaveo\Training\GSSHA\Calibration\Manual\id_map_4.idx" "soiltype"
ROUGHNESS "land use"
NUM_IDS 5
ID    DESCRIPTION1                            DESCRIPTION2                                   ROUGH
1     pine 27%                                                                            0.050541
2     water 0.3%                                                                          0.358000
3     cotton 14%                                                                          0.461467
4     pasture 42%                                                                         0.072003
5     gullied land 16%                                                                    0.971990
INTERCEPTION ""
NUM_IDS 0
ID    DESCRIPTION1                            DESCRIPTION2                               STOR_CAPY  INTER_COEF
RETENTION "land use"
NUM_IDS 5
ID    DESCRIPTION1                            DESCRIPTION2                            RETENTION_DEPTH
1     Pine 27%                                                                            1.504087
2     Water 0.3%                                                                          1.300000
3     Cotton 14%                                                                          1.013069
4     Pasture 42%                                                                         0.845919
5     Gullied land 16%                                                                    3.707182
GREEN_AMPT_INFILTRATION "lusoil"
NUM_IDS 9
ID    DESCRIPTION1                            DESCRIPTION2                               HYDR_COND  CAPIL_HEAD    POROSITY  PORE_INDEX   RESID_SAT FIELD_CAPACITY  WILTING_PT
1     gullied-land-silt-loam-15%                                                         3.331339  16.680000   0.486000   0.234000   0.015000   0.330000   0.133300
2     gullied-land-sand-1%                                                               1.410000   4.950000   0.437000   0.694000   0.020000   0.091000   0.033000
3     water-.3%                                                                          0.003000   0.003000   0.582000   0.001000   0.015000   0.436500   0.133300
4     pasture-clay-loam-3.5%                                                             0.019943  20.880000   0.464000   0.242000   0.075000   0.318000   0.133300
5     cotton-clay-loam-5%                                                                0.189387  20.880000   0.464000   0.242000   0.075000   0.318000   0.133300
6     pine-clay-loam-10%                                                                 0.292474  20.880000   0.464000   0.242000   0.075000   0.318000   0.133300
7     pine-silt-loam-17%                                                                 1.227514  16.680000   0.486000   0.234000   0.015000   0.330000   0.197000
8     cotton-silt-loam-9%                                                                2.693927  16.680000   0.486000   0.234000   0.015000   0.330000   0.133000
9     pasture-silt-loam-39%                                                              0.246209  16.680000   0.486000   0.234000   0.015000   0.330000   0.133000
GREEN_AMPT_INITIAL_SOIL_MOISTURE "lusoil"
NUM_IDS 9
ID    DESCRIPTION1                            DESCRIPTION2                            SOIL_MOISTURE
1     Soil moisture ID                                                                    0.330000
2     Soil moisture ID                                                                    0.150000
3     Soil moisture ID                                                                    0.150000
4     Soil moisture ID                                                                    0.150000
5     Soil moisture ID                                                                    0.318000
6     Soil moisture ID                                                                    0.318000
7     Soil moisture ID                                                                    0.330000
8     Soil moisture ID                                                                    0.330000
9     Soil moisture ID                                                                    0.330000
RICHARDS_EQN_INFILTRATION_BROOKS  ""
NUM_IDS 0
MAX_NUMBER_CELLS 0
ID    DESCRIPTION1                            DESCRIPTION2                                HYD_COND    POROSITY   RESID_SAT  SOIL_MOIST  WILTING_PT FIELD_CAPACITY       DEPTH      LAMBDA   BUB_PRESS     DELTA_Z
RICHARDS_EQN_INFILTRATION_HAVERCAMP  ""
NUM_IDS 0
MAX_NUMBER_CELLS 0
ID    DESCRIPTION1                            DESCRIPTION2                                HYD_COND    POROSITY   RESID_SAT  SOIL_MOIST  WILTING_PT FIELD_CAPACITY       DEPTH       ALPHA        BETA        AHAV        BHAV     DELTA_Z
EVAPOTRANSPIRATION "land use"
NUM_IDS 5
ID    DESCRIPTION1                            DESCRIPTION2                                  ALBEDO  VEG_HEIGHT  V_RAD_COEF CANOPY_RESIST
1     Pine                                                                                0.140000   10.000000    0.100000  120.000000
2     Water                                                                               0.050000    0.000100    1.000000 2000.000000
3     cotton                                                                              0.200000    1.000000    0.360000   17.000000
4     pasture                                                                             0.160000    0.500000    0.680000  100.000000
5     gullied land                                                                        0.230000    0.150000    0.800000  200.000000
SEDIMENTS
NUM_SED  0
Sediment Description                      Spec. Grav   Part. Dia     Output Filename
SOIL_EROSION_PROPS "lusoil"
NUM_IDS 9
NUM_SED 0
ID    DESCRIPTION1                            DESCRIPTION2                                 TC_COEFF     TC_INDEX      TC_CRIT     SPLASH_K DETACH_ERODE DETACH_INDEX  DETACH_CRIT        SED_K   0 SEDIMENTS....
1     Land ID #5, Cropland and Pasture       Soil ID #2, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.331200
2     Land ID #5, Cropland and Pasture       Soil ID #1, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.331200
3     Land ID #2, Residential                Soil ID #2, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.636100
4     Land ID #4, Residential                Soil ID #3, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.606100
5     Land ID #3, Deciduous Forest           Soil ID #3, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.606100
6     Land ID #1, Deciduous Forest           Soil ID #3, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.616200
7     Land ID #1, Transportation             Soil ID #2, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.616200
8     Land ID #3, Cropland and Pasture       Soil ID #2, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.616200
9     Land ID #4, Transportation             Soil ID #2, Untitled soiltype                0.285000    1.300000    0.000200 1200.000000    0.000100    0.400000    0.000000    0.616200
GROUNDWATER ""
NUM_IDS 0
ID    DESCRIPTION1                            DESCRIPTION2                                HYD_COND    POROSITY
WETLAND_PROPERTIES "wetlands"
NUM_IDS 0
ID                                                                                      INIT_DEPTH   RET_DEPTH RET_HYD_CON  VEG_HEIGHT VEG_HYD_CON   OVR_VEG_N
